Alta Moda Samples
peak-hard-knee

	Threshold
	Ratio
	Knee
	Attack
	Feedback
	Release

	7.5
	2
	hard
	Fast
	off
	2

	S.C. Insert
	Drive
	RMS/Peak
	Blend
	
	Output

	off
	off
	peak
	0
	
	5

	Filter
	Filter
	
	Filter
	
	

	
	off
	
	off
	
	


rms-soft-knee

	Threshold
	Ratio
	Knee
	Attack
	Feedback
	Release

	6.5
	2
	soft
	3
	off
	4

	S.C. Insert
	Drive
	RMS/Peak
	Blend
	
	Output

	off
	off
	rms
	0
	
	5

	Filter
	Filter
	
	Filter
	
	

	off
	off
	
	off
	
	


parallel-comp

	Threshold
	Ratio
	Knee
	Attack
	Feedback
	Release

	6
	2
	soft
	2
	off
	3

	S.C. Insert
	Drive
	RMS/Peak
	Blend
	
	Output

	off
	off
	rms
	1.5
	
	4

	Filter
	Filter
	
	Filter
	
	

	off
	off
	
	1
	
	


parallel-comp-with-drive

	Threshold
	Ratio
	Knee
	Attack
	Feedback
	Release

	6
	2
	soft
	2
	off
	3

	S.C. Insert
	Drive
	RMS/Peak
	Blend
	
	Output

	off
	3
	rms
	1.5
	
	4

	Filter
	Filter
	
	Filter
	
	

	off
	0
	
	1
	
	


